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[bookmark: _Hlk510607944]Lesson Plan: Health and Hazards (Welding Workshop)
Learning Outcome: 
Participants will become aware of health and hazards at the place of work, namely in work related to welding in a workshop.

Participants will watch a video (Health and Hazards – welding), identify hazards and analyse them. Video link: https://youtu.be/JOqNoiY-Crc 

Case Story:
  However keen on his work the worker is, he stills needs to handle the job better in all its aspects, especially correct H&S measures. At times he seems to learn from his own mistakes or takes belated actions, but that is not the way to go!
 
Teacher instructions:
Teacher asks students to watch video, taking note on the handout provided of any incorrect practices performed by the worker at the welding workshop. 

Students are asked to list all the incorrect work practices and other mistakes they can identify. On second viewing of the video, they need to ensure they have identified all flaws, even those that seem insignificant. If need be, a third run of the video is permitted to make sure all participants manage with the task. 

Finally, a class discussion is held about the points elicited, highlighting what one should do instead to adhere to correct practices at the workshop. Moreover, it would be of great benefit to rope in the consequences of such malpractices.

Main points included in Clip 2 (Health and Hazards in a welding workshop):

  Topics:
a) Reading of safety signs
b) Equipment must be of sufficient quality and safe (No breakages)
c) Welding with little protection against UV rays
d) Use of proper protection, gloves, overalls.
e) Use of ear defenders or plugs (someone else is working at the workshop banging and making noise)
f) Adequate light
g) Adequate ventilation
h) Handling of dirty material - wash hands frequently
i) Cleaning of hands (using soap not thinner)
j) Incorrect use of two pin socket in a BS1363 S/O
k) Switching off use of signs and locks
l) Recognise dangerous materials by reading labels not smell
m) Use of alcohol during working time.
Reinforcement:
Students are given a handout whereby they have to list the incorrect practices  at  the workplace. 
 
  A discussion of the points elicited is held after the final run of the video. 

How students would have worked were they doing the same job themselves should be discussed. 

Focus on the consequences of such incorrect practices should be made, for this will reinforce the learning process.
 
_ _ _ _ _
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Worksheet: Health and Hazards
Watch the video and make a list of flaws and incorrect practices related to work in a welding workshop. 

	Health and Hazards – in a welding workshop

	

	

	

	

	

	

	

	

	

	

	

	

	

	

	

	


 Reflective Questions
1. Which PPE would you recommend the worker should wear while working?
_____________________________________________________________________________________________________________________________________________________________________________________________

2. Which do you consider the three most serious mistakes the worker is making? Why?
___________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________
 
3. If you were on the spot, what advice would you have given the worker?
_____________________________________________________________________________________________________________________________________________________________________________________________

4. Some workers say: ”We don’t need any safety stuff; we know what we’re doing”. In view of this, how would you convince them to consider taking health and safety measures seriously?
_____________________________________________________________________________________________________________________________________________________________________________________________


[bookmark: _GoBack]Saħħa u Perikli (Health and hazards)    Clip 2
Clip 2  (Welding workshop)
[bookmark: _Hlk510708875]Topics:
n) Reading of safety signs
o) Equipment must be of sufficient quality and safe (No breakages)
p) Welding with little protection against UV rays
q) Use of proper protection, gloves, overalls.
r) Use of ear defenders or plugs (someone else is working at the workshop banging and doing noise)
s) Adequate light
t) Adequate ventilation
u) Handling of dirty material - wash hands frequently
v) Cleaning of hands (using soap not thinner)
w) Incorrect use of two pin socket in a BS1363 S/O
x) Switching off use of signs and locks
y) Recognise dangerous materials by reading labels not smell
z) Use of alcohol during working time.
Plot:
1. A worker entering a workshop without safety helmet cheering colleagues, but with safety notice requiring safety helmet behind. Man does not note signage
2. Man hangs coat against the nail holding the safety notice, hiding most of it.
3. Use basic welding protection like gloves, apron but uses T-shirt
4. Checks tools for maintenance and electrical integrity
5. Starts welding (his hand is exposed to UV light. Feels the effect and uses long sleeves
6. A colleague is banging on the anvil in the work shop (show hands only). Welder uses ear plugs
7. Welder has difficulty to see, so prepares a pilot lamp for better light.
8. Lack of ventilation
9. Pilot lamp has two pin plug. Uses a screw driver to bypass three pin plug shutter security system. It works ok
10. Welder stops for break
11. Has dirty hands
12. Needs to wash hands
a. Is undecided whether to use soap or thinner
b. Smells thinner but checks label on can
c. Sees hazard sign on thinner can 
d. Discards thinner and use soap
13. Eats his sandwich at the workshop and drinks a beer for his break.
14. Leaves lunch on work bench and goes to finish work
15. Leaves workplace with tools laying about, equipment on, etc.
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